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REQUEST FOR QUOTATION
	RFQ Reference: RFQ-30000031840
	Date: 25 August 2026

	Subject of RFQ: Request for Quotations for Procurement of 1-2 Units Fully Electric Vehicles (EVs)


International Organization for Migration kindly requests your quotation for the provision of the goods described in the RFQ submission form below and the attached technical requirements. This RFQ is not limited to price only; bidders must submit mandatory documentation and a completed technical compliance matrix for technical responsiveness review.
When preparing your quotation, please be guided by the RFQ information below. It is your responsibility to ensure that your quotation is submitted on or before the deadline. Quotations received after the submission deadline, for whatever reason, will not be considered for evaluation.
RFQ INFORMATION
	Deadline for the submission of quotation
	17th September 2026 At or Before 1000am East Africa Time
If any doubt exists as to the time zone in which the quotation should be submitted, refer to http://www.timeanddate.com/worldclock/.

	Method of submission
	Quotation must be submitted as follows: 
☒ E-tendering
☒ Email via iomnborfq@iom.int

	Cost of preparation of quotation
	IOM shall not be responsible for any costs associated with a vendor’s preparation and submission of a quotation, regardless of the outcome or the manner of conducting the selection process.

	Contractual Terms
	Any Purchase Order that will be issued as a result of this RFQ shall be subject to the IOM standard terms for provision of goods/services/transportation/medical services available at  or IOM standard contract templates.  

	Documents to be submitted
	Bidders shall submit and sign the-bid submission form below.

	Quotation validity period
	The quotation shall remain valid for 60 days from the deadline for the submission. 

	Price 
	Quotations shall be for the goods, works and/or services stated in the Specification/TOR/SOW 

	Partial quotations
	☒ Not permitted, unless IOM later decides to split award by unit quantity. Bidders should quote for both one-unit and two-unit options where possible.
☐ Permitted Insert conditions for partial bids and ensure that the requirements are properly listed in lots to allow partial bids

	Clarifications
	Contact person for correspondence, notifications and clarifications
Contact person: KCO Quotation Queries
E-mail address: KCO-Quotationqueries@iom.int

	Evaluation method
	☒ Lowest priced substantially compliant offer, subject to successful technical compliance review, mandatory documentation review, and IOM verification/clarification where required.

	Right not to accept any quotation
	IOM is not bound to accept any quotations, nor award a contract or purchase order

	Expected date for contract/PO award.
	Within 30 – 60 Days after the quotation closing day



Thank you and we look forward to receiving your quotation.
Issued by: Supply Chain Unit, IOM Kenya
Date:  	25/08/2026

Schedule of Requirements 
	Item No.
	Description
	UOM
	Qty

	1
	Supply, delivery and handover of new, unused, fully electric right-hand-drive Battery Electric Vehicle (BEV), compact/mid-size/practical full-size SUV or crossover, compliant with the minimum technical specifications in Annex A.
	Unit
	1-2


Purpose and Operational Context
IOM Kenya seeks to procure fully electric vehicle(s) for daily staff transportation, programme support activities, stakeholder engagements and peri-urban operations within the Nairobi Metropolitan Area.
The vehicle(s) must support IOM sustainability objectives while maintaining operational reliability under Kenyan road, climate and infrastructure conditions.
Preferred vehicle category: compact, mid-size or practical full-size BEV SUV/crossover suitable for routine Nairobi traffic, parking, staff transport and light operational support.
Mandatory Eligibility and Technical Submission Requirements
	Bidders must submit the documents below together with the financial quotation. Failure to submit adequate evidence for mandatory requirements may result in technical disqualification.


Completed and signed Quotation Submission Form, including price schedule for one-unit and two-unit options.
Completed Technical Compliance Matrix using Annex B, marked “Compliant”, “Partially Compliant” or “Non-Compliant” for each mandatory requirement, with references to supporting documents.
Manufacturer brochure and technical datasheet for the exact model offered.
Written warranty terms confirming battery, vehicle and powertrain warranty coverage.
Evidence of authorized or certified EV service support in Kenya, preferably Nairobi, including escalation contacts for warranty, technical support and spare parts requests.
Preventive maintenance schedule, recommended service intervals, estimated service costs and routine replacement parts list.
Spare parts support commitment for a minimum of eight (8) years from delivery, including expected lead times for non-stock spare parts.
Battery lifecycle, replacement and sustainability information, including replacement cost estimate, refurbishment options, recycling/end-of-life arrangements and projected battery availability for at least ten (10) years.
Mandatory vehicle documentation in English: Certificate of Origin, and Warranty Documentation.
Company Profile or Vendor Information Form, where not already registered or where details require update.
Signed Bidder’s Declaration of Conformity.
Minimum Technical Requirements Summary
	Area
	Minimum Requirement

	Vehicle configuration
	BEV; right-hand drive mandatory; minimum 5 doors; minimum 5 adult seating; 2WD minimum; AWD/4WD acceptable if efficient and operationally suitable; adequate cargo space, indicative 350-500 litres; 60:40 foldable rear seats; minimum 160 mm ground clearance; maximum 5.8 m turning radius.

	Dimensions
	Wheelbase sufficient for 5 adults, preferred 2,600-2,800 mm; preferred length 4,200-4,750 mm; vehicles exceeding 4,850 mm may be considered non-responsive unless justified and accepted by IOM; width minimum 1,750 mm and preferably not exceeding 1,950 mm; body must not be oversized/heavy-duty off-road style.

	Battery system
	Recognized EV battery chemistry such as LFP, NMC or equivalent; sufficient capacity for required range; preferred 50-80 kWh desirable only; suitable battery voltage; battery thermal management suitable for Kenyan climate; IP67 or equivalent battery protection; minimum 3,000 cycles preferred or certified durability meeting warranty/capacity retention.

	Range and efficiency
	Minimum WLTP range 350 km or demonstrated real-world operational range not less than 280 km under normal urban/peri-urban conditions; energy consumption not exceeding 18 kWh/100 km.

	Charging
	AC onboard charger minimum 7 kW; 11 kW preferred; Type 2 IEC 62196 or equivalent. DC fast charging suitable for operations, preferred minimum 65 kW; 80 kW preferred; CCS2 or equivalent; recognized IEC/CCS2 standards; 10-80% charging time preferably 45 minutes or less under compatible DC conditions.

	Warranty
	Battery warranty 8 years or 160,000 km with at least 70% capacity retention after warranty period; vehicle warranty 5 years or 100,000 km; powertrain warranty 8 years or 160,000 km.

	Roadworthiness and safety
	Independent front suspension; all-season radial tyres; spare wheel preferred or approved repair kit/inflator/equivalent; reinforced battery underbody protection; enhanced cabin filtration; minimum 5-star safety rating where available or equivalent safety compliance with documentation; ABS, ESC, traction control, hill hold, regenerative braking, airbags, rear parking sensors, reverse camera and TPMS/equivalent.

	Accessories
	USB charging ports, 12V accessory socket, first aid kit, fire extinguisher, reflective triangles, high-visibility safety vests, rubber floor mats, cargo cover and portable EV charging cable.

	Climate/environment
	Reliable operation from -10°C to +50°C, up to 95% relative humidity, altitude up to 2,500 m, enhanced dust sealing, automatic climate control, cabin air filtration and heat pump preferred.

	Delivery and handover
	Deliver to IOM Nairobi, Kenya; new, unused, fully assembled, cleaned, inspected and ready for operation; provide registration/customs/roadworthiness documents as applicable; conduct pre-delivery inspection and handover orientation on safe operation, charging, battery care, emergency procedures, warranty conditions, maintenance schedule and after-sales contacts.



Delivery Requirements: 
	Delivery Item
	Requirement

	Delivery period
	Bidder to confirm earliest delivery period upon issuance of Purchase Order.

	Delivery terms
	DAP IOM Nairobi, Kenya, unless otherwise agreed.

	Customs/importation and registration documentation
	Supplier/bidder to provide all documents required for registration and lawful operation in Kenya, including customs/import documents where applicable, certificate of origin, roadworthiness and registration documents and other documents required by Kenyan authorities.

	Pre-delivery inspection
	Supplier to provide signed pre-delivery inspection report confirming compliance, absence of visible defects and supply of all accessories, tools, manuals, charging cables, safety equipment, warranty documents and keys.

	Handover/basic training
	Supplier to conduct basic handover orientation covering safe operation, charging, battery care, emergency procedures, warranty conditions, maintenance schedule and after-sales contacts.











QUOTATION SUBMISSION FORM
	RFQ Reference: RFQ-30000031840
	Date: Click or tap to enter a date.


	Currency of the Quotation: USD/KES
INCOTERMS: DAP

	Item No
	Description
	UOM
	Qty
	Unit price
	Total price 

	1.
	Supply, delivery, registration support and handover of one (1) fully electric BEV SUV/crossover meeting Annex A specifications	Unit
	1
	
	

	2.
	Optional total price for two (2) identical units, inclusive of delivery, registration support and handover	Lot
	2
	
	

	Total Price
	

	Transportation Price, if not included above
	

	Insurance Price, if applicable
	

	Training, handover, orientation Price, if applicable
	

	Other Charges (specify)
	

	Total Final and All-inclusive Price
	




COMPANY PROFILE (Vendor Information Form)[footnoteRef:2]  [2:  If company id not registered in UNGM or with IOM. If supplied to IOM already, please indicate if there are any changes to be incorporated in the vendor information sheet signed earlier ] 

	Item Description
	Detail

	Legal name of bidder*
	Click or tap here to enter text.
	Legal Address (house no, street name, zip code, city*, region*, country*)
	Click or tap here to enter text.
	Website
	Click or tap here to enter text.
	Registration date* and VAT number*
	Click or tap here to enter text.	Click or tap here to enter text.

	Legal structure
	Choose an item.
	Business type/industry category* 
	☐ Direct Producer/Manufacturing    ☐ Reseller/Distributor/Service Provider

	Are you a UNGM registered vendor?
	☐ Yes  ☐ No            If yes, insert UNGM Vendor Number

	Do you provide services/goods internationally? 
	☐ Yes  ☐ No            If no, in which country: Click or tap here to enter text.

	Contact information* 
	Company Tel/Mobile: Click or tap here to enter text.
Company Email: Click or tap here to enter text.
Company Website: Click or tap here to enter text.
Contact Person 1:Click or tap here to enter text.
Contact Person 2: Click or tap here to enter text.

	Disability inclusive business*
	☐ Yes  ☐ No                    

	Women-owned/controlled*
	☐ Yes  ☐ No                    

	Bank Information
	Bank Name: Click or tap here to enter text.
Bank Address: Click or tap here to enter text.
IBAN: Click or tap here to enter text.
SWIFT/BIC: Click or tap here to enter text.
Account Currency: Click or tap here to enter text.
Bank Account Number: Click or tap here to enter text.	
Other relevant information: Click or tap here to enter text.



BIDDER’S DECLARATION OF CONFORMITY[footnoteRef:3] [3:  This form is mandatory to fill in and sign by every vendor who submits quotation ] 

	Yes
	No
	

	☐	☐	On behalf of the vendor, I hereby represent and warrant that neither the vendor, nor any person having powers of representation, decision-making or control over it or any member of its administrative, management or supervisory body, has been the subject of a final judgement or final administrative decision for one of the following reasons:  bankruptcy, insolvency or winding-up procedures; breach of obligations relating to the payment of taxes or social security contributions; grave professional misconduct, including misrepresentation, fraud; corruption; conduct related to a criminal organisation; money laundering or terrorist financing; terrorist offences or offences linked to terrorist activities; child labour and other trafficking in human beings, any discriminatory or exploitative practice, or any practice that is inconsistent with the rights set forth in the Convention on the Rights of the Child or other prohibited practices; irregularity; creating or being a shell company.

	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor is financially sound and duly licensed.


	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor has adequate human resources, equipment, competence, expertise and skills necessary to complete the contract fully and satisfactorily, within the stipulated completion period and in accordance with the relevant terms and conditions.


	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor complies with all applicable laws, ordinances, rules and regulations. 


	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor will in all circumstances act in the best interests of IOM.

	☐	☐	On behalf of the vendor, I further represent and warrant that no official of IOM or any third party has received from, will be offered by, or will receive from the vendor any direct or indirect benefit arising from the contract.


	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor has not misrepresented or concealed any material facts during the contracting process.


	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor will respect the legal status, privileges and immunities of IOM as an intergovernmental organization.


	☐	☐	On behalf of the vendor, I further represent and warrant that neither the vendor nor any persons having powers of representation, decision-making or control over the vendor or any member of its administrative, management or supervisory body are included in the most recent Consolidated United Nations Security Council Sanctions List (the “UN Sanctions List”) or are the subject of any sanctions or other temporary suspension. The vendor will immediately disclose to IOM if it or they become subject to any sanction or temporary suspension. 


	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor does not employ, provide resources to, support, contract or otherwise deal with any person, entity or other group associated with terrorism as per the UN Sanctions List and any other applicable anti-terrorism legislation.


	☐	☐	On behalf of the vendor, I further represent and warrant that, the vendor will apply the highest ethical standards, the principles of efficiency and economy, equal opportunity, open competition and transparency, and will avoid any conflict of interest. 


	☐	☐	On behalf of the vendor, I further represent and warrant that the vendor undertakes to comply with the Code of Conduct, available at https://www.ungm.org/Public/CodeOfConduct.


	☐	☐	It is the responsibility of the vendor to inform IOM immediately of any change to the information provided in this Declaration.

	☐	☐	On behalf of the vendor, I certify that I am duly authorized to sign this Declaration and on behalf of the vendor I agree to abide by the terms of this Declaration for the duration of any contract entered into between the vendor and IOM. 


	☐	☐	IOM reserves the right to terminate any contract between IOM and the vendor, with immediate effect and without liability, in the event of any misrepresentation made by the vendor in this Declaration.   





Signature: ____________________________

Name: 	Click or tap here to enter text.

Title:	Click or tap here to enter text.

Date:  	Click or tap to enter a date.














Annex A: Detailed Technical Specifications
	Bidders must treat mandatory requirements as pass/fail requirements. Preferred/desirable features are not mandatory unless expressly stated as mandatory.


	Specification Area
	Requirement

	Purpose/context
	Staff transportation, programme support, stakeholder engagements and peri-urban operations within Nairobi Metropolitan Area. Vehicle must be practical for Nairobi traffic/parking and light operational support.

	Vehicle type
	Battery Electric Vehicle (BEV).

	Steering
	Right-Hand Drive (mandatory).

	Doors/seats
	Minimum 5 doors; minimum 5 adults. 5-seat or practical full-size SUV/crossover acceptable; 7-seat may be considered if practical for Nairobi traffic and parking.

	Drive
	2WD minimum. AWD/4WD acceptable where offered without compromising efficiency, cost-effectiveness and Nairobi operational suitability.

	Cargo/rear seats
	Adequate luggage/cargo space; indicative preferred 350-500 litres. Rear seats foldable 60:40 split.

	Ground clearance/ turning radius
	Minimum 160 mm ground clearance. Maximum 5.8 m turning radius.

	Dimensions
	Preferred wheelbase 2,600-2,800 mm; preferred length 4,200-4,750 mm; exceeding 4,850 mm may be non-responsive unless justified/accepted; width minimum 1,750 mm and preferably not exceeding 1,950 mm excluding mirrors; height suitable for SUV/crossover, preferably 1,550-1,750 mm; not oversized/bulky/heavy-duty off-road style.

	Battery
	LFP, NMC or equivalent recognized chemistry; capacity sufficient for required range; preferred capacity 50-80 kWh desirable only; suitable manufacturer-standard voltage; active liquid thermal management preferred or equivalent; preconditioning preferred; IP67 or equivalent protection; 3,000 cycles preferred or certified durability.

	Range/consumption
	Minimum WLTP 350 km or demonstrated real-world range not less than 280 km under normal urban/peri-urban conditions; energy consumption ≤18 kWh/100 km.

	AC charging
	Minimum 7 kW onboard charger; 11 kW preferred; Type 2 (IEC 62196) or equivalent connector.

	DC charging
	DC fast charging suitable for operational use; preferred minimum 65 kW; ≥80 kW preferred; CCS2 or equivalent connector; IEC 61851/IEC 62196/CCS2 or equivalent recognized standards; 10-80% preferably ≤45 minutes where compatible.

	Warranty
	Battery warranty 8 years or 160,000 km; capacity retention ≥70% after warranty; vehicle warranty 5 years or 100,000 km; powertrain warranty 8 years or 160,000 km. Written warranty terms required.

	Battery lifecycle
	Provide replacement cost estimate, refurbishment options, recycling arrangements, end-of-life management plan, environmental compliance/carbon footprint/battery sourcing information where available. Replacement battery cost should not exceed 30% of vehicle acquisition cost. Current pricing and projected availability for at least 10 years required.

	Roadworthiness
	Independent front suspension; multi-link rear preferred; all-season radial tyres; full-size spare wheel preferred or approved repair kit/inflator/roadside puncture support; reinforced battery protection; enhanced cabin filtration.

	Safety
	Minimum 5-star safety rating where available from Euro NCAP, ANCAP, Global NCAP or equivalent certified compliance. Mandatory: ABS, ESC, traction control, hill hold assist, regenerative braking, front/side/curtain airbags, rear parking sensors, reverse camera, TPMS or equivalent.

	Accessories
	USB ports, 12V socket, first aid kit, fire extinguisher, reflective triangles, high-visibility vests, rubber floor mats, cargo cover and portable EV charging cable.

	Climate/HVAC
	Operate from -10°C to +50°C, humidity up to 95%, altitude up to 2,500 m, enhanced dust sealing. Automatic climate control, cabin air filtration and heat pump preferred.

	After-sales support
	Authorized/certified EV service centre in Kenya, preferably Nairobi; trained EV technicians and escalation contacts; spare parts availability in Kenya or defined arrangement; 48-hour technical support response; eight-year spare parts support; critical spare parts support; preventive maintenance schedule and lead times for non-stock parts.

	Delivery/handover
	Deliver to IOM Nairobi, new, unused, fully assembled, cleaned, inspected and ready. Provide registration/lawful operation documents; pre-delivery inspection; handover orientation/basic training.



Annex B: Technical Compliance Matrix
	Bidders must complete this matrix. IOM may request clarification, additional evidence, physical inspection, demonstration, or verification prior to award.


	No.
	Requirement
	Bidder Compliance
	Evidence / Document Reference

	1
	BEV, right-hand drive, minimum 5 doors and minimum 5 adult seating
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	2
	Suitable compact/mid-size/practical full-size SUV/crossover for Nairobi operations, not oversized/heavy-duty off-road style
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	3
	Minimum 160 mm ground clearance and maximum 5.8 m turning radius
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	4
	Minimum WLTP range 350 km or demonstrated real-world range ≥280 km
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	5
	Energy consumption ≤18 kWh/100 km
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	6
	AC charging minimum 7 kW and Type 2 or equivalent connector
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	7
	DC fast charging with CCS2 or equivalent compatible connector
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	8
	Battery warranty 8 years/160,000 km and ≥70% capacity retention
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	9
	Vehicle warranty 5 years/100,000 km and powertrain warranty 8 years/160,000 km
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	10
	IP67 or equivalent battery protection and reinforced battery underbody protection
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	11
	Mandatory safety features: ABS/ESC/traction control/hill hold/regenerative braking/airbags/rear sensors/reverse camera/TPMS or equivalent
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	12
	Mandatory accessories supplied
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	13
	Vehicle suitable for -10°C to +50°C, up to 95% humidity and up to 2,500 m altitude
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	14
	Mandatory documents in English supplied in printed and electronic PDF copies
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	15
	Authorized/certified EV service support in Kenya, preferably Nairobi
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	16
	48-hour technical support response and eight-year spare parts support commitment
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	17
	Battery lifecycle/replacement/recycling/end-of-life information provided
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	18
	Delivery to IOM Nairobi with registration/lawful operation documents and pre-delivery inspection report
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
	

	19
	Handover orientation/basic EV training included
	☐ Compliant  ☐ Partially Compliant       ☐ Non-Compliant
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